{"text_format":"1","workbook":"xlsx","n_sheets":3,"sheets":["CFG","LPG","K151"],"not_rendered":{"charts":0,"images":0,"macros":1,"external_links":0,"defined_names":12,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"CFG","index":0,"n_rows":7,"n_cols":6,"rows_kept":7,"cut":false,"hidden":true,"merged":[]}
["Cesta pro uložení:","\\\\sunpchmplp01.ug.cz\\CRC\\Kontrol_listy\\",null,null,null,"cptVS"]
["Jméno souboru:","Pojist_ventily_P3"]
["Rozšíření jména:","YYMMDDHHmm"]
["Formát pro uloření:",43,"56 - Excel 97-2003"]
["Extenze pro uloření:","xlsm","xlsx"]
["Změna v sešitu","A"]
[null,"S:\\Vitek\\cpt\\"]

{"sheet":"LPG","index":1,"n_rows":56,"n_cols":4,"rows_kept":56,"cut":false,"hidden":false,"merged":[[34,1,35,1],[36,1,37,1],[38,1,39,1],[0,0,0,3],[26,1,27,1],[28,1,29,1],[30,1,31,1],[32,1,33,1],[18,1,19,1],[20,1,21,1],[22,1,23,1],[24,1,25,1],[5,1,6,1],[8,1,9,1],[11,1,12,1],[14,1,15,1]]}
["Kontrolní list poj.ventilů Bl.64 LPG"]
[]
["označení","kde","stav","poznámky"]
["6410-RV001","dusík na R-tank - na zdi venku"]
["6420-RV001","sání P1 -nad H01","OK"]
["6420-RV001A","H 01","OK"]
["6420-RV001B",null,"OK"]
["6420-RV002","sání P2 -mezi H44/45","OK"]
["6420-RV002A","H 02","OK"]
["6420-RV002B",null,"OK"]
["6420-RV003","sání P3 -nad H45","OK"]
["6420-RV003A","H 03","OK"]
["6420-RV003B",null,"OK"]
["6420-RV004","H01-03 na k.151 - gal. u č.s.","OK"]
["6420-RV004A","H 04","OK"]
["6420-RV004B",null,"OK"]
["6420-RV005","výtlak P2/4 na PCHII -nad kond.n.","uzavřen","nepoužívá se"]
["6420-RV006","výtlak na PS18 - gal. u č.s.","Ano"]
["6420-RV007A","E 05","Ano"]
["6420-RV007B",null,"Ano"]
["6420-RV024A","H 36","Ano"]
["6420-RV024B",null,"Ano"]
["6420-RV025A","H 37","Ano"]
["6420-RV025B",null,"Ano"]
["6420-RV026A","H 38","Ano"]
["6420-RV026B",null,"Ano"]
["6420-RV027A","H 39","Ano"]
["6420-RV027B",null,"Ano"]
["6420-RV028A","H 40","Ano"]
["6420-RV028B",null,"Ano"]
["6420-RV029A","H 41","Ano"]
["6420-RV029B",null,"Ano"]
["6420-RV030A","H 42","Ano"]
["6420-RV030B",null,"Ano"]
["6420-RV031A","H 43","Ano"]
["6420-RV031B",null,"Ano"]
["6420-RV032A","H 44","Ano"]
["6420-RV032B",null,"Ano"]
["6420-RV033A","H 45","Ano"]
["6420-RV033B",null,"Ano"]
["6420-RV034","H40-45 do blendru... ,mezi H44/45","Ano"]
["6420-RV035","dusík na LPG -konec mostu dole u H04","zdemontován","komínek"]
["6420-RV045","H 82 - vzdušník","Ano"]
["6420-RV170/4","LPG na PCH II - most170/kor.","Ano"]
["6420-TERV008","sání P4 -nad H45","Ano"]
["6420-TERV036","C4/PS18 do skladu -nad H44","Ano"]
["6420-TERV037","PB AVD -nad kond.n.","Ano"]
["6420-TERV038","k.151 do skladu -nad H43","Ano"]
["6420-TERV039","C3/PS18 do skladu -nad kond.n.","Ano"]
["6420-TERV040","PB NRL do skladu -mezi H43/44","Ano"]
["6420-TERV041","sání z H 37 do H38/39 - nad H 37","Ano"]
["6420-TERV042","výtlak P2/4 na PCHII u \"Ja\"mostu","Ano"]
[]
[]
[null,"kontroloval:","Směna D - vit"]
[null,"datum:","2026-03-05T09:10:42"]

{"sheet":"K151","index":2,"n_rows":30,"n_cols":4,"rows_kept":30,"cut":false,"hidden":false,"merged":[[0,0,0,2]]}
["Kontrolní list poj.ventilů Bl.55 K151"]
[]
["označení","kde","stav","poznámky"]
["5520-RV002","vzdušník k.151","OK"]
["5520-RV003","C4 do ŽC -před reg.v.","OK"]
["5520-RV004","C5 ŽC proplach - mezi reg.v.","OK"]
["5520-RV005","C3/C4 na ŽC -mezi reg.v.","OK"]
["5520-RV006","C5 na ŽC -mezi reg.v.","OK"]
["5520-RV007","H61 -ř.12, pravý","OK"]
["5520-RV009","C3 na AC -mezi reg.v.","OK"]
["5520-RV010","H51 -ř.12","OK"]
["5520-RV011","H51 -ř.12","OK"]
["5520-RV012","C3 na AC -před reg.v.","OK"]
["5520-RV013","C5 na ŽC -před  reg.v.","OK"]
["5520-RV014","C3 na ŽC -před reg.v.","OK"]
["5520-RV015","H51/61 do H37 -nahoře nad kond.n.","OK"]
["5520-RV016","H 61 -ř.12, levý","OK"]
["5520-RV017","E 06","OK"]
["5520-RV018","E 06","OK"]
["5520-RV022","výtlak čerpadla etanolu","OK"]
["5520-RV048","C3/C4 na ŽC -za reg.v.","OK"]
["5520-TERV019","stáčení z ŽC -před chladičem","OK"]
["5520-TERV020","stáčení z ŽC -výtlak P05","OK"]
["5520-TERV021","C4 do E 06 -před reg.v. E06","OK"]
["5520-TERV046","C3 na AC -za reg.v.","OK"]
["5520-TERV047","C5 na ŽC -za reg.v.","OK"]
["5520-TERV049","stáčení z ŽC -výtlak P05, za U Z281","OK"]
[]
[null,"Kontroloval:"]
[null,"datum:"]